// This is the SIP interface definition for TQDataView.
//
// Copyright (c) 2007
// 	Riverbank Computing Limited <info@riverbankcomputing.co.uk>
// 
// This file is part of PyTQt.
// 
// This copy of PyTQt is free software; you can redistribute it and/or modify it
// under the terms of the GNU General Public License as published by the Free
// Software Foundation; either version 2, or (at your option) any later
// version.
// 
// PyTQt is supplied in the hope that it will be useful, but WITHOUT ANY
// WARRANTY; without even the implied warranty of MERCHANTABILITY or FITNESS
// FOR A PARTICULAR PURPOSE.  See the GNU General Public License for more
// details.
// 
// You should have received a copy of the GNU General Public License along with
// PyTQt; see the file LICENSE.  If not, write to the Free Software Foundation,
// Inc., 59 Temple Place - Suite 330, Boston, MA 02111-1307, USA.


%ExportedDoc
<Sect2><Title>TQDataView (TQt v3+)</Title>
<Para>
<Literal>TQDataView</Literal> is fully implemented.
</Para>
</Sect2>
%End


%If (TQt_3_0_0 -)

class TQDataView : TQWidget
{
%TypeHeaderCode
#include <tqdataview.h>
%End

public:
	TQDataView(TQWidget * /TransferThis/ = 0,const char * = 0,WFlags = 0);

	virtual void setForm(TQSqlForm *);
	TQSqlForm *form();
	virtual void setRecord(TQSqlRecord *);
	TQSqlRecord *record();

public slots:
	virtual void refresh(TQSqlRecord *);
	virtual void readFields();
	virtual void writeFields();
	virtual void clearValues();

private:
%If (TQt_3_1_0 -)
	TQDataView(const TQDataView &);
%End
};

%End
